 -- Copyright (C) 1991-2007 Altera Corporation
 -- Your use of Altera Corporation's design tools, logic functions 
 -- and other software and tools, and its AMPP partner logic 
 -- functions, and any output files from any of the foregoing 
 -- (including device programming or simulation files), and any 
 -- associated documentation or information are expressly subject 
 -- to the terms and conditions of the Altera Program License 
 -- Subscription Agreement, Altera MegaCore Function License 
 -- Agreement, or other applicable license agreement, including, 
 -- without limitation, that your use is for the sole purpose of 
 -- programming logic devices manufactured by Altera and sold by 
 -- Altera or its authorized distributors.  Please refer to the 
 -- applicable agreement for further details.
 -- 
 -- This is a Quartus II output file. It is for reporting purposes only, and is
 -- not intended for use as a Quartus II input file. This file cannot be used
 -- to make Quartus II pin assignments - for instructions on how to make pin
 -- assignments, please see Quartus II help.
 ---------------------------------------------------------------------------------



 ---------------------------------------------------------------------------------
 -- NC            : No Connect. This pin has no internal connection to the device.
 -- DNU           : Do Not Use. This pin MUST NOT be connected.
 -- VCCPGM        : Dedicated power pin for configuration, which MUST be connected to 1.8V, 2.5V or 3.0V depending on the needs of the configuration device.
 -- VCCINT        : Dedicated power pin, which MUST be connected to VCC  (1.2V).
 -- VCCIO         : Dedicated power pin, which MUST be connected to VCC
 --                 of its bank.
 --					Bank 1:		3.3V
 --					Bank 2:		3.3V
 --					Bank 3:		3.3V
 --					Bank 4:		3.3V
 --					Bank 5:		3.3V
 --					Bank 6:		3.3V
 --					Bank 7:		3.3V
 --					Bank 8:		3.3V
 -- GND           : Dedicated ground pin. Dedicated GND pins MUST be connected to GND.
 --					It can also be used to report unused dedicated pins. The connection
 --					on the board for unused dedicated pins depends on whether this will
 --					be used in a future design. One example is device migration. When
 --					using device migration, refer to the device pin-tables. If it is a
 --					GND pin in the pin table or if it will not be used in a future design
 --					for another purpose the it MUST be connected to GND. If it is an unused
 --					dedicated pin, then it can be connected to a valid signal on the board
 --					(low, high, or toggling) if that signal is required for a different
 --					revision of the design.
 -- GND+          : Unused input pin. It can also be used to report unused dual-purpose pins.
 --					This pin should be connected to GND. It may also be connected  to a
 --					valid signal  on the board  (low, high, or toggling)  if that signal
 --					is required for a different revision of the design.
 -- GND*          : Unused  I/O  pin.   For transceiver I/O banks (Bank 13, 14, 15, 16 and 17),
 --           	    connect each pin marked GND* either individually through a 10 kohm resistor
 --           	    to GND or tie all pins together and connect through a single 10 kohm resistor
 --           	    to GND.
 --           	    For non-transceiver I/O banks, connect each pin marked GND* directly to GND
 --           	    or leave it unconnected.
 -- RESERVED      : Unused I/O pin, which MUST be left unconnected.
 -- RESERVED_INPUT    : Pin is tri-stated and should be connected to the board.
 -- RESERVED_INPUT_WITH_WEAK_PULLUP    : Pin is tri-stated with internal weak pull-up resistor.
 -- RESERVED_INPUT_WITH_BUS_HOLD       : Pin is tri-stated with bus-hold circuitry.
 -- RESERVED_OUTPUT_DRIVEN_HIGH        : Pin is output driven high.
 ---------------------------------------------------------------------------------



 ---------------------------------------------------------------------------------
 -- Pin directions (input, output or bidir) are based on device operating in user mode.
 ---------------------------------------------------------------------------------

Quartus II Version 7.2 Build 207 03/18/2008 Service Pack 3 SJ Full Version
CHIP  "DE2_70_D5M_XVGA"  ASSIGNED TO AN: EP2C70F896C6

Pin Name/Usage               : Location  : Dir.   : I/O Standard      : Voltage : I/O Bank  : User Assignment
-------------------------------------------------------------------------------------------------------------
GND                          : A2        : gnd    :                   :         :           :                
iTD1_D[6]                    : A3        : input  : 3.3-V LVTTL       :         : 3         : Y              
VCCIO3                       : A4        : power  :                   : 3.3V    : 3         :                
iTD1_D[2]                    : A5        : input  : 3.3-V LVTTL       :         : 3         : Y              
iTD1_D[0]                    : A6        : input  : 3.3-V LVTTL       :         : 3         : Y              
iTD2_D[6]                    : A7        : input  : 3.3-V LVTTL       :         : 3         : Y              
iTD2_D[4]                    : A8        : input  : 3.3-V LVTTL       :         : 3         : Y              
iTD2_D[1]                    : A9        : input  : 3.3-V LVTTL       :         : 3         : Y              
oVGA_G[0]                    : A10       : output : 3.3-V LVTTL       :         : 3         : Y              
oVGA_G[2]                    : A11       : output : 3.3-V LVTTL       :         : 3         : Y              
oVGA_G[5]                    : A12       : output : 3.3-V LVTTL       :         : 3         : Y              
GND                          : A13       : gnd    :                   :         :           :                
oVGA_G[9]                    : A14       : output : 3.3-V LVTTL       :         : 3         : Y              
VCCIO3                       : A15       : power  :                   : 3.3V    : 3         :                
VCCIO4                       : A16       : power  :                   : 3.3V    : 4         :                
oVGA_B[2]                    : A17       : output : 3.3-V LVTTL       :         : 4         : Y              
GND                          : A18       : gnd    :                   :         :           :                
oVGA_B[7]                    : A19       : output : 3.3-V LVTTL       :         : 4         : Y              
ENET_D[7]                    : A20       : bidir  : 3.3-V LVTTL       :         : 4         : Y              
ENET_D[5]                    : A21       : bidir  : 3.3-V LVTTL       :         : 4         : Y              
ENET_D[3]                    : A22       : bidir  : 3.3-V LVTTL       :         : 4         : Y              
ENET_D[0]                    : A23       : bidir  : 3.3-V LVTTL       :         : 4         : Y              
ENET_D[14]                   : A24       : bidir  : 3.3-V LVTTL       :         : 4         : Y              
ENET_D[11]                   : A25       : bidir  : 3.3-V LVTTL       :         : 4         : Y              
ENET_D[9]                    : A26       : bidir  : 3.3-V LVTTL       :         : 4         : Y              
VCCIO4                       : A27       : power  :                   : 3.3V    : 4         :                
oENET_IOR_N                  : A28       : output : 3.3-V LVTTL       :         : 4         : Y              
GND                          : A29       : gnd    :                   :         :           :                
DRAM_DQ[27]                  : AA1       : bidir  : 3.3-V LVTTL       :         : 1         : Y              
DRAM_DQ[28]                  : AA2       : bidir  : 3.3-V LVTTL       :         : 1         : Y              
DRAM_DQ[29]                  : AA3       : bidir  : 3.3-V LVTTL       :         : 1         : Y              
oDRAM0_A[0]                  : AA4       : output : 3.3-V LVTTL       :         : 1         : Y              
oDRAM0_A[1]                  : AA5       : output : 3.3-V LVTTL       :         : 1         : Y              
oDRAM0_A[2]                  : AA6       : output : 3.3-V LVTTL       :         : 1         : Y              
GND*                         : AA7       :        :                   :         : 1         :                
oDRAM0_CKE                   : AA8       : output : 3.3-V LVTTL       :         : 1         : Y              
oDRAM0_BA[0]                 : AA9       : output : 3.3-V LVTTL       :         : 1         : Y              
oDRAM0_BA[1]                 : AA10      : output : 3.3-V LVTTL       :         : 1         : Y              
GND                          : AA11      : gnd    :                   :         :           :                
GND                          : AA12      : gnd    :                   :         :           :                
VCCINT                       : AA13      : power  :                   : 1.2V    :           :                
VCCINT                       : AA14      : power  :                   : 1.2V    :           :                
GND                          : AA15      : gnd    :                   :         :           :                
GND                          : AA16      : gnd    :                   :         :           :                
VCCINT                       : AA17      : power  :                   : 1.2V    :           :                
VCCINT                       : AA18      : power  :                   : 1.2V    :           :                
GND                          : AA19      : gnd    :                   :         :           :                
GND                          : AA20      : gnd    :                   :         :           :                
GND_PLL4                     : AA21      : gnd    :                   :         :           :                
GND_PLL4                     : AA22      : gnd    :                   :         :           :                
iSW[0]                       : AA23      : input  : 3.3-V LVTTL       :         : 6         : Y              
oLEDG[7]                     : AA24      : output : 3.3-V LVTTL       :         : 6         : Y              
GND*                         : AA25      :        :                   :         : 6         :                
GND*                         : AA26      :        :                   :         : 6         :                
oLEDG[6]                     : AA27      : output : 3.3-V LVTTL       :         : 6         : Y              
GND*                         : AA28      :        :                   :         : 6         :                
FLASH_DQ[6]                  : AA29      : bidir  : 3.3-V LVTTL       :         : 6         : Y              
FLASH_DQ[14]                 : AA30      : bidir  : 3.3-V LVTTL       :         : 6         : Y              
DRAM_DQ[30]                  : AB1       : bidir  : 3.3-V LVTTL       :         : 1         : Y              
DRAM_DQ[31]                  : AB2       : bidir  : 3.3-V LVTTL       :         : 1         : Y              
VCCIO1                       : AB3       : power  :                   : 3.3V    : 1         :                
GND                          : AB4       : gnd    :                   :         :           :                
oDRAM0_A[3]                  : AB5       : output : 3.3-V LVTTL       :         : 1         : Y              
oDRAM0_UDQM1                 : AB6       : output : 3.3-V LVTTL       :         : 1         : Y              
oDRAM0_A[4]                  : AB7       : output : 3.3-V LVTTL       :         : 1         : Y              
GND_PLL1                     : AB8       : gnd    :                   :         :           :                
VCCD_PLL1                    : AB9       : power  :                   : 1.2V    :           :                
GND                          : AB10      : gnd    :                   :         :           :                
VCCIO8                       : AB11      : power  :                   : 3.3V    : 8         :                
oLEDR[13]                    : AB12      : output : 3.3-V LVTTL       :         : 8         : Y              
oLEDR[11]                    : AB13      : output : 3.3-V LVTTL       :         : 8         : Y              
GND                          : AB14      : gnd    :                   :         :           :                
VCCIO8                       : AB15      : power  :                   : 3.3V    : 8         :                
VCCIO7                       : AB16      : power  :                   : 3.3V    : 7         :                
GND                          : AB17      : gnd    :                   :         :           :                
oHEX2_D[4]                   : AB18      : output : 3.3-V LVTTL       :         : 7         : Y              
oHEX2_D[5]                   : AB19      : output : 3.3-V LVTTL       :         : 7         : Y              
VCCIO7                       : AB20      : power  :                   : 3.3V    : 7         :                
GND                          : AB21      : gnd    :                   :         :           :                
VCCD_PLL4                    : AB22      : power  :                   : 1.2V    :           :                
GND*                         : AB23      :        :                   :         : 6         :                
GND*                         : AB24      :        :                   :         : 6         :                
iSW[2]                       : AB25      : input  : 3.3-V LVTTL       :         : 6         : Y              
iSW[1]                       : AB26      : input  : 3.3-V LVTTL       :         : 6         : Y              
GND                          : AB27      : gnd    :                   :         :           :                
VCCIO6                       : AB28      : power  :                   : 3.3V    : 6         :                
FLASH_DQ[5]                  : AB29      : bidir  : 3.3-V LVTTL       :         : 6         : Y              
FLASH_DQ[13]                 : AB30      : bidir  : 3.3-V LVTTL       :         : 6         : Y              
DRAM_DQ[0]                   : AC1       : bidir  : 3.3-V LVTTL       :         : 1         : Y              
DRAM_DQ[1]                   : AC2       : bidir  : 3.3-V LVTTL       :         : 1         : Y              
DRAM_DQ[2]                   : AC3       : bidir  : 3.3-V LVTTL       :         : 1         : Y              
oDRAM0_A[5]                  : AC4       : output : 3.3-V LVTTL       :         : 1         : Y              
oDRAM0_A[6]                  : AC5       : output : 3.3-V LVTTL       :         : 1         : Y              
oDRAM0_A[7]                  : AC6       : output : 3.3-V LVTTL       :         : 1         : Y              
oDRAM0_A[9]                  : AC7       : output : 3.3-V LVTTL       :         : 1         : Y              
GND_PLL1                     : AC8       : gnd    :                   :         :           :                
VCCA_PLL1                    : AC9       : power  :                   : 1.2V    :           :                
GNDA_PLL1                    : AC10      : gnd    :                   :         :           :                
oLEDR[14]                    : AC11      : output : 3.3-V LVTTL       :         : 8         : Y              
oLEDR[12]                    : AC12      : output : 3.3-V LVTTL       :         : 8         : Y              
oLEDR[10]                    : AC13      : output : 3.3-V LVTTL       :         : 8         : Y              
oLEDG[8]                     : AC14      : output : 3.3-V LVTTL       :         : 8         : Y              
GND+                         : AC15      :        :                   :         : 7         :                
oSRAM_A[14]                  : AC16      : output : 3.3-V LVTTL       :         : 7         : Y              
oHEX1_DP                     : AC17      : output : 3.3-V LVTTL       :         : 7         : Y              
oSRAM_ADSP_N                 : AC18      : output : 3.3-V LVTTL       :         : 7         : Y              
oHEX2_DP                     : AC19      : output : 3.3-V LVTTL       :         : 7         : Y              
oSRAM_BE_N[1]                : AC20      : output : 3.3-V LVTTL       :         : 7         : Y              
oSRAM_BE_N[0]                : AC21      : output : 3.3-V LVTTL       :         : 7         : Y              
VCCA_PLL4                    : AC22      : power  :                   : 1.2V    :           :                
iSW[6]                       : AC23      : input  : 3.3-V LVTTL       :         : 6         : Y              
iSW[5]                       : AC24      : input  : 3.3-V LVTTL       :         : 6         : Y              
GND*                         : AC25      :        :                   :         : 6         :                
iSW[4]                       : AC26      : input  : 3.3-V LVTTL       :         : 6         : Y              
iSW[3]                       : AC27      : input  : 3.3-V LVTTL       :         : 6         : Y              
FLASH_DQ[11]                 : AC28      : bidir  : 3.3-V LVTTL       :         : 6         : Y              
FLASH_DQ[4]                  : AC29      : bidir  : 3.3-V LVTTL       :         : 6         : Y              
FLASH_DQ[12]                 : AC30      : bidir  : 3.3-V LVTTL       :         : 6         : Y              
DRAM_DQ[3]                   : AD1       : bidir  : 3.3-V LVTTL       :         : 1         : Y              
DRAM_DQ[4]                   : AD2       : bidir  : 3.3-V LVTTL       :         : 1         : Y              
DRAM_DQ[5]                   : AD3       : bidir  : 3.3-V LVTTL       :         : 1         : Y              
oDRAM0_A[8]                  : AD4       : output : 3.3-V LVTTL       :         : 1         : Y              
GND*                         : AD5       :        :                   :         : 1         :                
oDRAM0_CLK                   : AD6       : output : 3.3-V LVTTL       :         : 1         : Y              
oSRAM_CLK                    : AD7       : output : 3.3-V LVTTL       :         : 1         : Y              
oLEDR[16]                    : AD8       : output : 3.3-V LVTTL       :         : 8         : Y              
oLEDR[15]                    : AD9       : output : 3.3-V LVTTL       :         : 8         : Y              
oHEX0_D[3]                   : AD10      : output : 3.3-V LVTTL       :         : 8         : Y              
oHEX0_D[5]                   : AD11      : output : 3.3-V LVTTL       :         : 8         : Y              
oHEX0_D[6]                   : AD12      : output : 3.3-V LVTTL       :         : 8         : Y              
oSRAM_A[8]                   : AD13      : output : 3.3-V LVTTL       :         : 8         : Y              
oLEDR[9]                     : AD14      : output : 3.3-V LVTTL       :         : 8         : Y              
iCLK_50                      : AD15      : input  : 3.3-V LVTTL       :         : 7         : Y              
oSRAM_ADV_N                  : AD16      : output : 3.3-V LVTTL       :         : 7         : Y              
oHEX1_D[6]                   : AD17      : output : 3.3-V LVTTL       :         : 7         : Y              
oSRAM_OE_N                   : AD18      : output : 3.3-V LVTTL       :         : 7         : Y              
GND*                         : AD19      :        :                   :         : 7         :                
oSRAM_BE_N[2]                : AD20      : output : 3.3-V LVTTL       :         : 7         : Y              
oFLASH_A[18]                 : AD21      : output : 3.3-V LVTTL       :         : 7         : Y              
oSRAM_CE3_N                  : AD22      : output : 3.3-V LVTTL       :         : 7         : Y              
GNDA_PLL4                    : AD23      : gnd    :                   :         :           :                
iSW[8]                       : AD24      : input  : 3.3-V LVTTL       :         : 6         : Y              
iSW[7]                       : AD25      : input  : 3.3-V LVTTL       :         : 6         : Y              
GND*                         : AD26      :        :                   :         : 6         :                
GND*                         : AD27      :        :                   :         : 6         :                
GND*                         : AD28      :        :                   :         : 6         :                
FLASH_DQ[10]                 : AD29      : bidir  : 3.3-V LVTTL       :         : 6         : Y              
FLASH_DQ[3]                  : AD30      : bidir  : 3.3-V LVTTL       :         : 6         : Y              
DRAM_DQ[6]                   : AE1       : bidir  : 3.3-V LVTTL       :         : 1         : Y              
DRAM_DQ[7]                   : AE2       : bidir  : 3.3-V LVTTL       :         : 1         : Y              
DRAM_DQ[8]                   : AE3       : bidir  : 3.3-V LVTTL       :         : 1         : Y              
oDRAM0_A[11]                 : AE4       : output : 3.3-V LVTTL       :         : 1         : Y              
VCCIO1                       : AE5       : power  :                   : 3.3V    : 1         :                
GND                          : AE6       : gnd    :                   :         :           :                
oHEX2_D[0]                   : AE7       : output : 3.3-V LVTTL       :         : 8         : Y              
oHEX0_D[0]                   : AE8       : output : 3.3-V LVTTL       :         : 8         : Y              
GND                          : AE9       : gnd    :                   :         :           :                
VCCIO8                       : AE10      : power  :                   : 3.3V    : 8         :                
oSRAM_A[17]                  : AE11      : output : 3.3-V LVTTL       :         : 8         : Y              
oSRAM_A[6]                   : AE12      : output : 3.3-V LVTTL       :         : 8         : Y              
oSRAM_A[9]                   : AE13      : output : 3.3-V LVTTL       :         : 8         : Y              
GND                          : AE14      : gnd    :                   :         :           :                
oSRAM_A[12]                  : AE15      : output : 3.3-V LVTTL       :         : 8         : Y              
oHEX1_D[1]                   : AE16      : output : 3.3-V LVTTL       :         : 7         : Y              
oHEX1_D[4]                   : AE17      : output : 3.3-V LVTTL       :         : 7         : Y              
GND                          : AE18      : gnd    :                   :         :           :                
oHEX2_D[6]                   : AE19      : output : 3.3-V LVTTL       :         : 7         : Y              
oFLASH_A[21]                 : AE20      : output : 3.3-V LVTTL       :         : 7         : Y              
VCCIO7                       : AE21      : power  :                   : 3.3V    : 7         :                
GND                          : AE22      : gnd    :                   :         :           :                
oFLASH_A[2]                  : AE23      : output : 3.3-V LVTTL       :         : 7         : Y              
FLASH_DQ15_AM1               : AE24      : bidir  : 3.3-V LVTTL       :         : 7         : Y              
GND                          : AE25      : gnd    :                   :         :           :                
VCCIO6                       : AE26      : power  :                   : 3.3V    : 6         :                
iSW[9]                       : AE27      : input  : 3.3-V LVTTL       :         : 6         : Y              
FLASH_DQ[1]                  : AE28      : bidir  : 3.3-V LVTTL       :         : 6         : Y              
FLASH_DQ[9]                  : AE29      : bidir  : 3.3-V LVTTL       :         : 6         : Y              
FLASH_DQ[2]                  : AE30      : bidir  : 3.3-V LVTTL       :         : 6         : Y              
DRAM_DQ[9]                   : AF1       : bidir  : 3.3-V LVTTL       :         : 1         : Y              
DRAM_DQ[10]                  : AF2       : bidir  : 3.3-V LVTTL       :         : 1         : Y              
DRAM_DQ[11]                  : AF3       : bidir  : 3.3-V LVTTL       :         : 1         : Y              
oDRAM0_A[12]                 : AF4       : output : 3.3-V LVTTL       :         : 1         : Y              
GND                          : AF5       : gnd    :                   :         :           :                
VCCIO8                       : AF6       : power  :                   : 3.3V    : 8         :                
oHEX2_D[1]                   : AF7       : output : 3.3-V LVTTL       :         : 8         : Y              
oSRAM_A[1]                   : AF8       : output : 3.3-V LVTTL       :         : 8         : Y              
oHEX0_D[1]                   : AF9       : output : 3.3-V LVTTL       :         : 8         : Y              
oHEX0_D[4]                   : AF10      : output : 3.3-V LVTTL       :         : 8         : Y              
oSRAM_A[18]                  : AF11      : output : 3.3-V LVTTL       :         : 8         : Y              
oHEX0_DP                     : AF12      : output : 3.3-V LVTTL       :         : 8         : Y              
VCCIO8                       : AF13      : power  :                   : 3.3V    : 8         :                
oSRAM_A[10]                  : AF14      : output : 3.3-V LVTTL       :         : 8         : Y              
oSRAM_A[13]                  : AF15      : output : 3.3-V LVTTL       :         : 8         : Y              
oHEX1_D[2]                   : AF16      : output : 3.3-V LVTTL       :         : 7         : Y              
oHEX1_D[5]                   : AF17      : output : 3.3-V LVTTL       :         : 7         : Y              
oSRAM_WE_N                   : AF18      : output : 3.3-V LVTTL       :         : 7         : Y              
VCCIO7                       : AF19      : power  :                   : 3.3V    : 7         :                
oSRAM_A[15]                  : AF20      : output : 3.3-V LVTTL       :         : 7         : Y              
oFLASH_A[17]                 : AF21      : output : 3.3-V LVTTL       :         : 7         : Y              
oFLASH_A[7]                  : AF22      : output : 3.3-V LVTTL       :         : 7         : Y              
oFLASH_A[4]                  : AF23      : output : 3.3-V LVTTL       :         : 7         : Y              
oFLASH_A[0]                  : AF24      : output : 3.3-V LVTTL       :         : 7         : Y              
VCCIO7                       : AF25      : power  :                   : 3.3V    : 7         :                
GND                          : AF26      : gnd    :                   :         :           :                
GPIO_CLKOUT_N1               : AF27      : bidir  : 3.3-V LVTTL       :         : 6         : Y              
GPIO_CLKOUT_P1               : AF28      : bidir  : 3.3-V LVTTL       :         : 6         : Y              
FLASH_DQ[0]                  : AF29      : bidir  : 3.3-V LVTTL       :         : 6         : Y              
FLASH_DQ[8]                  : AF30      : bidir  : 3.3-V LVTTL       :         : 6         : Y              
VCCIO1                       : AG1       : power  :                   : 3.3V    : 1         :                
DRAM_DQ[12]                  : AG2       : bidir  : 3.3-V LVTTL       :         : 1         : Y              
DRAM_DQ[13]                  : AG3       : bidir  : 3.3-V LVTTL       :         : 1         : Y              
oHEX2_D[3]                   : AG4       : output : 3.3-V LVTTL       :         : 8         : Y              
oSRAM_A[5]                   : AG5       : output : 3.3-V LVTTL       :         : 8         : Y              
oSRAM_A[4]                   : AG6       : output : 3.3-V LVTTL       :         : 8         : Y              
oSRAM_A[3]                   : AG7       : output : 3.3-V LVTTL       :         : 8         : Y              
oSRAM_A[0]                   : AG8       : output : 3.3-V LVTTL       :         : 8         : Y              
GND*                         : AG9       :        :                   :         : 8         :                
GND*                         : AG10      :        :                   :         : 8         :                
GND                          : AG11      : gnd    :                   :         :           :                
oSRAM_A[7]                   : AG12      : output : 3.3-V LVTTL       :         : 8         : Y              
oHEX1_D[0]                   : AG13      : output : 3.3-V LVTTL       :         : 8         : Y              
oSRAM_A[11]                  : AG14      : output : 3.3-V LVTTL       :         : 8         : Y              
GPIO_CLKIN_P1                : AG15      : input  : 3.3-V LVTTL       :         : 8         : Y              
oHEX1_D[3]                   : AG16      : output : 3.3-V LVTTL       :         : 7         : Y              
oSRAM_ADSC_N                 : AG17      : output : 3.3-V LVTTL       :         : 7         : Y              
oSRAM_GW_N                   : AG18      : output : 3.3-V LVTTL       :         : 7         : Y              
oSRAM_CE2                    : AG19      : output : 3.3-V LVTTL       :         : 7         : Y              
oSRAM_A[16]                  : AG20      : output : 3.3-V LVTTL       :         : 7         : Y              
GND                          : AG21      : gnd    :                   :         :           :                
oFLASH_A[5]                  : AG22      : output : 3.3-V LVTTL       :         : 7         : Y              
oFLASH_A[3]                  : AG23      : output : 3.3-V LVTTL       :         : 7         : Y              
oFLASH_A[1]                  : AG24      : output : 3.3-V LVTTL       :         : 7         : Y              
oFLASH_A[16]                 : AG25      : output : 3.3-V LVTTL       :         : 7         : Y              
GND*                         : AG26      :        :                   :         : 7         :                
GND*                         : AG27      :        :                   :         : 7         :                
oFLASH_CE_N                  : AG28      : output : 3.3-V LVTTL       :         : 6         : Y              
oFLASH_OE_N                  : AG29      : output : 3.3-V LVTTL       :         : 6         : Y              
VCCIO6                       : AG30      : power  :                   : 3.3V    : 6         :                
DRAM_DQ[14]                  : AH1       : bidir  : 3.3-V LVTTL       :         : 1         : Y              
DRAM_DQ[15]                  : AH2       : bidir  : 3.3-V LVTTL       :         : 1         : Y              
oLEDR[8]                     : AH3       : output : 3.3-V LVTTL       :         : 8         : Y              
oLEDR[5]                     : AH4       : output : 3.3-V LVTTL       :         : 8         : Y              
oHEX2_D[2]                   : AH5       : output : 3.3-V LVTTL       :         : 8         : Y              
GND                          : AH6       : gnd    :                   :         :           :                
oSRAM_A[2]                   : AH7       : output : 3.3-V LVTTL       :         : 8         : Y              
VCCIO8                       : AH8       : power  :                   : 3.3V    : 8         :                
oHEX0_D[2]                   : AH9       : output : 3.3-V LVTTL       :         : 8         : Y              
SRAM_DQ[0]                   : AH10      : bidir  : 3.3-V LVTTL       :         : 8         : Y              
VCCIO8                       : AH11      : power  :                   : 3.3V    : 8         :                
SRAM_DQ[5]                   : AH12      : bidir  : 3.3-V LVTTL       :         : 8         : Y              
SRAM_DQ[27]                  : AH13      : bidir  : 3.3-V LVTTL       :         : 8         : Y              
GPIO_CLKIN_N1                : AH14      : input  : 3.3-V LVTTL       :         : 8         : Y              
SRAM_DQ[21]                  : AH15      : bidir  : 3.3-V LVTTL       :         : 8         : Y              
SRAM_DQ[7]                   : AH16      : bidir  : 3.3-V LVTTL       :         : 7         : Y              
SRAM_DQ[10]                  : AH17      : bidir  : 3.3-V LVTTL       :         : 7         : Y              
SRAM_DQ[12]                  : AH18      : bidir  : 3.3-V LVTTL       :         : 7         : Y              
oSRAM_CE1_N                  : AH19      : output : 3.3-V LVTTL       :         : 7         : Y              
oSRAM_BE_N[3]                : AH20      : output : 3.3-V LVTTL       :         : 7         : Y              
VCCIO7                       : AH21      : power  :                   : 3.3V    : 7         :                
oFLASH_A[6]                  : AH22      : output : 3.3-V LVTTL       :         : 7         : Y              
VCCIO7                       : AH23      : power  :                   : 3.3V    : 7         :                
oFLASH_A[15]                 : AH24      : output : 3.3-V LVTTL       :         : 7         : Y              
GND                          : AH25      : gnd    :                   :         :           :                
oFLASH_A[10]                 : AH26      : output : 3.3-V LVTTL       :         : 7         : Y              
oFLASH_A[8]                  : AH27      : output : 3.3-V LVTTL       :         : 7         : Y              
oFLASH_RST_N                 : AH28      : output : 3.3-V LVTTL       :         : 6         : Y              
oFLASH_WP_N                  : AH29      : output : 3.3-V LVTTL       :         : 6         : Y              
iFLASH_RY_N                  : AH30      : input  : 3.3-V LVTTL       :         : 6         : Y              
GND                          : AJ1       : gnd    :                   :         :           :                
oLEDR[7]                     : AJ2       : output : 3.3-V LVTTL       :         : 8         : Y              
oLEDR[6]                     : AJ3       : output : 3.3-V LVTTL       :         : 8         : Y              
oLEDR[3]                     : AJ4       : output : 3.3-V LVTTL       :         : 8         : Y              
oLEDR[2]                     : AJ5       : output : 3.3-V LVTTL       :         : 8         : Y              
oLEDR[0]                     : AJ6       : output : 3.3-V LVTTL       :         : 8         : Y              
oLEDR[17]                    : AJ7       : output : 3.3-V LVTTL       :         : 8         : Y              
SRAM_DQ[30]                  : AJ8       : bidir  : 3.3-V LVTTL       :         : 8         : Y              
SRAM_DPA[3]                  : AJ9       : bidir  : 3.3-V LVTTL       :         : 8         : Y              
SRAM_DQ[1]                   : AJ10      : bidir  : 3.3-V LVTTL       :         : 8         : Y              
SRAM_DQ[3]                   : AJ11      : bidir  : 3.3-V LVTTL       :         : 8         : Y              
SRAM_DQ[6]                   : AJ12      : bidir  : 3.3-V LVTTL       :         : 8         : Y              
SRAM_DQ[26]                  : AJ13      : bidir  : 3.3-V LVTTL       :         : 8         : Y              
SRAM_DQ[25]                  : AJ14      : bidir  : 3.3-V LVTTL       :         : 8         : Y              
SRAM_DQ[22]                  : AJ15      : bidir  : 3.3-V LVTTL       :         : 8         : Y              
SRAM_DQ[23]                  : AJ16      : bidir  : 3.3-V LVTTL       :         : 7         : Y              
SRAM_DQ[9]                   : AJ17      : bidir  : 3.3-V LVTTL       :         : 7         : Y              
SRAM_DQ[11]                  : AJ18      : bidir  : 3.3-V LVTTL       :         : 7         : Y              
SRAM_DQ[14]                  : AJ19      : bidir  : 3.3-V LVTTL       :         : 7         : Y              
SRAM_DQ[16]                  : AJ20      : bidir  : 3.3-V LVTTL       :         : 7         : Y              
SRAM_DQ[18]                  : AJ21      : bidir  : 3.3-V LVTTL       :         : 7         : Y              
SRAM_DQ[20]                  : AJ22      : bidir  : 3.3-V LVTTL       :         : 7         : Y              
SRAM_DPA[1]                  : AJ23      : bidir  : 3.3-V LVTTL       :         : 7         : Y              
GND*                         : AJ24      :        :                   :         : 7         :                
oFLASH_A[13]                 : AJ25      : output : 3.3-V LVTTL       :         : 7         : Y              
oFLASH_A[11]                 : AJ26      : output : 3.3-V LVTTL       :         : 7         : Y              
oFLASH_A[9]                  : AJ27      : output : 3.3-V LVTTL       :         : 7         : Y              
oFLASH_A[20]                 : AJ28      : output : 3.3-V LVTTL       :         : 7         : Y              
oFLASH_WE_N                  : AJ29      : output : 3.3-V LVTTL       :         : 6         : Y              
GND                          : AJ30      : gnd    :                   :         :           :                
GND                          : AK2       : gnd    :                   :         :           :                
oLEDR[4]                     : AK3       : output : 3.3-V LVTTL       :         : 8         : Y              
VCCIO8                       : AK4       : power  :                   : 3.3V    : 8         :                
oLEDR[1]                     : AK5       : output : 3.3-V LVTTL       :         : 8         : Y              
GND*                         : AK6       :        :                   :         : 8         :                
SRAM_DQ[29]                  : AK7       : bidir  : 3.3-V LVTTL       :         : 8         : Y              
SRAM_DQ[31]                  : AK8       : bidir  : 3.3-V LVTTL       :         : 8         : Y              
SRAM_DPA[0]                  : AK9       : bidir  : 3.3-V LVTTL       :         : 8         : Y              
SRAM_DQ[2]                   : AK10      : bidir  : 3.3-V LVTTL       :         : 8         : Y              
SRAM_DQ[4]                   : AK11      : bidir  : 3.3-V LVTTL       :         : 8         : Y              
SRAM_DQ[28]                  : AK12      : bidir  : 3.3-V LVTTL       :         : 8         : Y              
GND                          : AK13      : gnd    :                   :         :           :                
SRAM_DQ[24]                  : AK14      : bidir  : 3.3-V LVTTL       :         : 8         : Y              
VCCIO8                       : AK15      : power  :                   : 3.3V    : 8         :                
VCCIO7                       : AK16      : power  :                   : 3.3V    : 7         :                
SRAM_DQ[8]                   : AK17      : bidir  : 3.3-V LVTTL       :         : 7         : Y              
GND                          : AK18      : gnd    :                   :         :           :                
SRAM_DQ[13]                  : AK19      : bidir  : 3.3-V LVTTL       :         : 7         : Y              
SRAM_DPA[2]                  : AK20      : bidir  : 3.3-V LVTTL       :         : 7         : Y              
SRAM_DQ[17]                  : AK21      : bidir  : 3.3-V LVTTL       :         : 7         : Y              
SRAM_DQ[19]                  : AK22      : bidir  : 3.3-V LVTTL       :         : 7         : Y              
SRAM_DQ[15]                  : AK23      : bidir  : 3.3-V LVTTL       :         : 7         : Y              
GND*                         : AK24      :        :                   :         : 7         :                
oFLASH_A[14]                 : AK25      : output : 3.3-V LVTTL       :         : 7         : Y              
oFLASH_A[12]                 : AK26      : output : 3.3-V LVTTL       :         : 7         : Y              
VCCIO7                       : AK27      : power  :                   : 3.3V    : 7         :                
oFLASH_A[19]                 : AK28      : output : 3.3-V LVTTL       :         : 7         : Y              
GND                          : AK29      : gnd    :                   :         :           :                
GND                          : B1        : gnd    :                   :         :           :                
LCD_D[7]                     : B2        : bidir  : 3.3-V LVTTL       :         : 2         : Y              
iTD1_D[7]                    : B3        : input  : 3.3-V LVTTL       :         : 3         : Y              
iTD1_D[4]                    : B4        : input  : 3.3-V LVTTL       :         : 3         : Y              
iTD1_D[3]                    : B5        : input  : 3.3-V LVTTL       :         : 3         : Y              
iTD1_D[1]                    : B6        : input  : 3.3-V LVTTL       :         : 3         : Y              
iTD2_D[7]                    : B7        : input  : 3.3-V LVTTL       :         : 3         : Y              
iTD2_D[5]                    : B8        : input  : 3.3-V LVTTL       :         : 3         : Y              
iTD2_D[2]                    : B9        : input  : 3.3-V LVTTL       :         : 3         : Y              
oTD2_RESET_N                 : B10       : output : 3.3-V LVTTL       :         : 3         : Y              
oVGA_G[1]                    : B11       : output : 3.3-V LVTTL       :         : 3         : Y              
oVGA_G[4]                    : B12       : output : 3.3-V LVTTL       :         : 3         : Y              
oVGA_G[7]                    : B13       : output : 3.3-V LVTTL       :         : 3         : Y              
oVGA_G[8]                    : B14       : output : 3.3-V LVTTL       :         : 3         : Y              
oVGA_SYNC_N                  : B15       : output : 3.3-V LVTTL       :         : 3         : Y              
oVGA_B[0]                    : B16       : output : 3.3-V LVTTL       :         : 4         : Y              
oVGA_B[3]                    : B17       : output : 3.3-V LVTTL       :         : 4         : Y              
oVGA_B[5]                    : B18       : output : 3.3-V LVTTL       :         : 4         : Y              
oVGA_B[6]                    : B19       : output : 3.3-V LVTTL       :         : 4         : Y              
ENET_D[6]                    : B20       : bidir  : 3.3-V LVTTL       :         : 4         : Y              
ENET_D[4]                    : B21       : bidir  : 3.3-V LVTTL       :         : 4         : Y              
ENET_D[2]                    : B22       : bidir  : 3.3-V LVTTL       :         : 4         : Y              
ENET_D[15]                   : B23       : bidir  : 3.3-V LVTTL       :         : 4         : Y              
ENET_D[13]                   : B24       : bidir  : 3.3-V LVTTL       :         : 4         : Y              
ENET_D[10]                   : B25       : bidir  : 3.3-V LVTTL       :         : 4         : Y              
ENET_D[8]                    : B26       : bidir  : 3.3-V LVTTL       :         : 4         : Y              
oENET_CMD                    : B27       : output : 3.3-V LVTTL       :         : 4         : Y              
oENET_IOW_N                  : B28       : output : 3.3-V LVTTL       :         : 4         : Y              
oENET_RESET_N                : B29       : output : 3.3-V LVTTL       :         : 4         : Y              
GND                          : B30       : gnd    :                   :         :           :                
LCD_D[4]                     : C1        : bidir  : 3.3-V LVTTL       :         : 2         : Y              
LCD_D[5]                     : C2        : bidir  : 3.3-V LVTTL       :         : 2         : Y              
LCD_D[6]                     : C3        : bidir  : 3.3-V LVTTL       :         : 2         : Y              
iTD1_D[5]                    : C4        : input  : 3.3-V LVTTL       :         : 3         : Y              
GND*                         : C5        :        :                   :         : 3         :                
GND                          : C6        : gnd    :                   :         :           :                
GND*                         : C7        :        :                   :         : 3         :                
VCCIO3                       : C8        : power  :                   : 3.3V    : 3         :                
iTD2_D[3]                    : C9        : input  : 3.3-V LVTTL       :         : 3         : Y              
iTD2_D[0]                    : C10       : input  : 3.3-V LVTTL       :         : 3         : Y              
VCCIO3                       : C11       : power  :                   : 3.3V    : 3         :                
oVGA_G[3]                    : C12       : output : 3.3-V LVTTL       :         : 3         : Y              
oVGA_G[6]                    : C13       : output : 3.3-V LVTTL       :         : 3         : Y              
GND*                         : C14       :        :                   :         : 3         :                
oVGA_BLANK_N                 : C15       : output : 3.3-V LVTTL       :         : 3         : Y              
oVGA_B[1]                    : C16       : output : 3.3-V LVTTL       :         : 4         : Y              
GND*                         : C17       :        :                   :         : 4         :                
oVGA_B[4]                    : C18       : output : 3.3-V LVTTL       :         : 4         : Y              
oVGA_B[8]                    : C19       : output : 3.3-V LVTTL       :         : 4         : Y              
VCCIO4                       : C20       : power  :                   : 3.3V    : 4         :                
GND*                         : C21       :        :                   :         : 4         :                
ENET_D[1]                    : C22       : bidir  : 3.3-V LVTTL       :         : 4         : Y              
VCCIO4                       : C23       : power  :                   : 3.3V    : 4         :                
ENET_D[12]                   : C24       : bidir  : 3.3-V LVTTL       :         : 4         : Y              
GND                          : C25       : gnd    :                   :         :           :                
GND*                         : C26       :        :                   :         : 4         :                
iENET_INT                    : C27       : input  : 3.3-V LVTTL       :         : 4         : Y              
oENET_CS_N                   : C28       : output : 3.3-V LVTTL       :         : 4         : Y              
GPIO_0[1]                    : C29       : bidir  : 3.3-V LVTTL       :         : 5         : Y              
GPIO_0[0]                    : C30       : bidir  : 3.3-V LVTTL       :         : 5         : Y              
VCCIO2                       : D1        : power  :                   : 3.3V    : 2         :                
LCD_D[2]                     : D2        : bidir  : 3.3-V LVTTL       :         : 2         : Y              
LCD_D[3]                     : D3        : bidir  : 3.3-V LVTTL       :         : 2         : Y              
OTG_D[8]                     : D4        : bidir  : 3.3-V LVTTL       :         : 3         : Y              
OTG_D[9]                     : D5        : bidir  : 3.3-V LVTTL       :         : 3         : Y              
OTG_D[10]                    : D6        : bidir  : 3.3-V LVTTL       :         : 3         : Y              
OTG_D[12]                    : D7        : bidir  : 3.3-V LVTTL       :         : 3         : Y              
oOTG_A[1]                    : D8        : output : 3.3-V LVTTL       :         : 3         : Y              
OTG_D[14]                    : D9        : bidir  : 3.3-V LVTTL       :         : 3         : Y              
oOTG_OE_N                    : D10       : output : 3.3-V LVTTL       :         : 3         : Y              
GND                          : D11       : gnd    :                   :         :           :                
oOTG_DACK0_N                 : D12       : output : 3.3-V LVTTL       :         : 3         : Y              
GND*                         : D13       :        :                   :         : 3         :                
oTD1_RESET_N                 : D14       : output : 3.3-V LVTTL       :         : 3         : Y              
iTD2_VS                      : D15       : input  : 3.3-V LVTTL       :         : 3         : Y              
iCLK_50_2                    : D16       : input  : 3.3-V LVTTL       :         : 4         : Y              
oAUD_XCK                     : D17       : output : 3.3-V LVTTL       :         : 4         : Y              
GND*                         : D18       :        :                   :         : 4         :                
oVGA_B[9]                    : D19       : output : 3.3-V LVTTL       :         : 4         : Y              
GND                          : D20       : gnd    :                   :         :           :                
iUART_RXD                    : D21       : input  : 3.3-V LVTTL       :         : 4         : Y              
oVGA_R[3]                    : D22       : output : 3.3-V LVTTL       :         : 4         : Y              
oVGA_R[0]                    : D23       : output : 3.3-V LVTTL       :         : 4         : Y              
oVGA_CLOCK                   : D24       : output : 3.3-V LVTTL       :         : 4         : Y              
PS2_MSDAT                    : D25       : bidir  : 3.3-V LVTTL       :         : 4         : Y              
PS2_MSCLK                    : D26       : bidir  : 3.3-V LVTTL       :         : 4         : Y              
oENET_CLK                    : D27       : output : 3.3-V LVTTL       :         : 4         : Y              
GPIO_0[5]                    : D28       : bidir  : 3.3-V LVTTL       :         : 5         : Y              
GPIO_0[3]                    : D29       : bidir  : 3.3-V LVTTL       :         : 5         : Y              
VCCIO5                       : D30       : power  :                   : 3.3V    : 5         :                
LCD_D[0]                     : E1        : bidir  : 3.3-V LVTTL       :         : 2         : Y              
oLCD_EN                      : E2        : output : 3.3-V LVTTL       :         : 2         : Y              
LCD_D[1]                     : E3        : bidir  : 3.3-V LVTTL       :         : 2         : Y              
oHEX6_D[6]                   : E4        : output : 3.3-V LVTTL       :         : 2         : Y              
GND                          : E5        : gnd    :                   :         :           :                
VCCIO3                       : E6        : power  :                   : 3.3V    : 3         :                
OTG_D[11]                    : E7        : bidir  : 3.3-V LVTTL       :         : 3         : Y              
OTG_D[13]                    : E8        : bidir  : 3.3-V LVTTL       :         : 3         : Y              
oOTG_A[0]                    : E9        : output : 3.3-V LVTTL       :         : 3         : Y              
oOTG_CS_N                    : E10       : output : 3.3-V LVTTL       :         : 3         : Y              
oOTG_WE_N                    : E11       : output : 3.3-V LVTTL       :         : 3         : Y              
oOTG_DACK1_N                 : E12       : output : 3.3-V LVTTL       :         : 3         : Y              
iTD1_HS                      : E13       : input  : 3.3-V LVTTL       :         : 3         : Y              
iTD1_VS                      : E14       : input  : 3.3-V LVTTL       :         : 3         : Y              
iTD2_HS                      : E15       : input  : 3.3-V LVTTL       :         : 3         : Y              
iCLK_28                      : E16       : input  : 3.3-V LVTTL       :         : 4         : Y              
AUD_BCLK                     : E17       : bidir  : 3.3-V LVTTL       :         : 4         : Y              
VCCIO4                       : E18       : power  :                   : 3.3V    : 4         :                
iAUD_ADCDAT                  : E19       : input  : 3.3-V LVTTL       :         : 4         : Y              
oVGA_R[8]                    : E20       : output : 3.3-V LVTTL       :         : 4         : Y              
oUART_TXD                    : E21       : output : 3.3-V LVTTL       :         : 4         : Y              
oVGA_R[2]                    : E22       : output : 3.3-V LVTTL       :         : 4         : Y              
oVGA_R[1]                    : E23       : output : 3.3-V LVTTL       :         : 4         : Y              
PS2_KBDAT                    : E24       : bidir  : 3.3-V LVTTL       :         : 4         : Y              
VCCIO4                       : E25       : power  :                   : 3.3V    : 4         :                
GND                          : E26       : gnd    :                   :         :           :                
GPIO_0[4]                    : E27       : bidir  : 3.3-V LVTTL       :         : 5         : Y              
GPIO_0[2]                    : E28       : bidir  : 3.3-V LVTTL       :         : 5         : Y              
GPIO_0[6]                    : E29       : bidir  : 3.3-V LVTTL       :         : 5         : Y              
GPIO_0[8]                    : E30       : bidir  : 3.3-V LVTTL       :         : 5         : Y              
oLCD_ON                      : F1        : output : 3.3-V LVTTL       :         : 2         : Y              
oLCD_RS                      : F2        : output : 3.3-V LVTTL       :         : 2         : Y              
oLCD_RW                      : F3        : output : 3.3-V LVTTL       :         : 2         : Y              
oHEX6_D[5]                   : F4        : output : 3.3-V LVTTL       :         : 2         : Y              
VCCIO2                       : F5        : power  :                   : 3.3V    : 2         :                
GND                          : F6        : gnd    :                   :         :           :                
OTG_FSPEED                   : F7        : bidir  : 3.3-V LVTTL       :         : 3         : Y              
OTG_LSPEED                   : F8        : bidir  : 3.3-V LVTTL       :         : 3         : Y              
GND                          : F9        : gnd    :                   :         :           :                
VCCIO3                       : F10       : power  :                   : 3.3V    : 3         :                
OTG_D[3]                     : F11       : bidir  : 3.3-V LVTTL       :         : 3         : Y              
iOTG_DREQ1                   : F12       : input  : 3.3-V LVTTL       :         : 3         : Y              
iOTG_INT0                    : F13       : input  : 3.3-V LVTTL       :         : 3         : Y              
GND                          : F14       : gnd    :                   :         :           :                
VCCIO3                       : F15       : power  :                   : 3.3V    : 3         :                
GND*                         : F16       :        :                   :         : 4         :                
GND                          : F17       : gnd    :                   :         :           :                
oAUD_DACDAT                  : F18       : output : 3.3-V LVTTL       :         : 4         : Y              
AUD_ADCLRCK                  : F19       : bidir  : 3.3-V LVTTL       :         : 4         : Y              
oVGA_R[7]                    : F20       : output : 3.3-V LVTTL       :         : 4         : Y              
VCCIO4                       : F21       : power  :                   : 3.3V    : 4         :                
GND                          : F22       : gnd    :                   :         :           :                
iUART_RTS                    : F23       : input  : 3.3-V LVTTL       :         : 4         : Y              
PS2_KBCLK                    : F24       : bidir  : 3.3-V LVTTL       :         : 4         : Y              
GND                          : F25       : gnd    :                   :         :           :                
VCCIO5                       : F26       : power  :                   : 3.3V    : 5         :                
GND*                         : F27       :        :                   :         : 5         :                
GND*                         : F28       :        :                   :         : 5         :                
GPIO_0[10]                   : F29       : bidir  : 3.3-V LVTTL       :         : 5         : Y              
GPIO_0[12]                   : F30       : bidir  : 3.3-V LVTTL       :         : 5         : Y              
oHEX7_D[6]                   : G1        : output : 3.3-V LVTTL       :         : 2         : Y              
oHEX7_DP                     : G2        : output : 3.3-V LVTTL       :         : 2         : Y              
oLCD_BLON                    : G3        : output : 3.3-V LVTTL       :         : 2         : Y              
oHEX6_D[4]                   : G4        : output : 3.3-V LVTTL       :         : 2         : Y              
oDRAM1_CLK                   : G5        : output : 3.3-V LVTTL       :         : 2         : Y              
GND*                         : G6        :        :                   :         : 2         :                
~ASDO~ / RESERVED_INPUT_WITH_WEAK_PULLUP : G7        : input  : 3.3-V LVTTL       :         : 2         : N              
GNDA_PLL3                    : G8        : gnd    :                   :         :           :                
OTG_D[1]                     : G9        : bidir  : 3.3-V LVTTL       :         : 3         : Y              
OTG_D[15]                    : G10       : bidir  : 3.3-V LVTTL       :         : 3         : Y              
OTG_D[2]                     : G11       : bidir  : 3.3-V LVTTL       :         : 3         : Y              
iOTG_DREQ0                   : G12       : input  : 3.3-V LVTTL       :         : 3         : Y              
OTG_D[7]                     : G13       : bidir  : 3.3-V LVTTL       :         : 3         : Y              
GND*                         : G14       :        :                   :         : 3         :                
iTD1_CLK27                   : G15       : input  : 3.3-V LVTTL       :         : 3         : Y              
GND*                         : G16       :        :                   :         : 4         :                
GND*                         : G17       :        :                   :         : 4         :                
AUD_DACLRCK                  : G18       : bidir  : 3.3-V LVTTL       :         : 4         : Y              
GND*                         : G19       :        :                   :         : 4         :                
oVGA_R[9]                    : G20       : output : 3.3-V LVTTL       :         : 4         : Y              
oVGA_R[5]                    : G21       : output : 3.3-V LVTTL       :         : 4         : Y              
oUART_CTS                    : G22       : output : 3.3-V LVTTL       :         : 4         : Y              
GNDA_PLL2                    : G23       : gnd    :                   :         :           :                
GPIO_CLKOUT_P0               : G24       : bidir  : 3.3-V LVTTL       :         : 5         : Y              
GPIO_0[7]                    : G25       : bidir  : 3.3-V LVTTL       :         : 5         : Y              
GPIO_0[9]                    : G26       : bidir  : 3.3-V LVTTL       :         : 5         : Y              
GPIO_1[0]                    : G27       : bidir  : 3.3-V LVTTL       :         : 5         : Y              
GPIO_1[1]                    : G28       : bidir  : 3.3-V LVTTL       :         : 5         : Y              
GPIO_0[11]                   : G29       : bidir  : 3.3-V LVTTL       :         : 5         : Y              
GPIO_0[13]                   : G30       : bidir  : 3.3-V LVTTL       :         : 5         : Y              
oHEX7_D[3]                   : H1        : output : 3.3-V LVTTL       :         : 2         : Y              
oHEX7_D[4]                   : H2        : output : 3.3-V LVTTL       :         : 2         : Y              
oHEX7_D[5]                   : H3        : output : 3.3-V LVTTL       :         : 2         : Y              
oHEX6_D[1]                   : H4        : output : 3.3-V LVTTL       :         : 2         : Y              
GND*                         : H5        :        :                   :         : 2         :                
oHEX6_D[0]                   : H6        : output : 3.3-V LVTTL       :         : 2         : Y              
oHEX6_D[2]                   : H7        : output : 3.3-V LVTTL       :         : 2         : Y              
oHEX6_D[3]                   : H8        : output : 3.3-V LVTTL       :         : 2         : Y              
VCCA_PLL3                    : H9        : power  :                   : 1.2V    :           :                
OTG_D[0]                     : H10       : bidir  : 3.3-V LVTTL       :         : 3         : Y              
GND*                         : H11       :        :                   :         : 3         :                
OTG_D[5]                     : H12       : bidir  : 3.3-V LVTTL       :         : 3         : Y              
OTG_D[6]                     : H13       : bidir  : 3.3-V LVTTL       :         : 3         : Y              
oOTG_RESET_N                 : H14       : output : 3.3-V LVTTL       :         : 3         : Y              
iTD2_CLK27                   : H15       : input  : 3.3-V LVTTL       :         : 3         : Y              
GND*                         : H16       :        :                   :         : 4         :                
GND*                         : H17       :        :                   :         : 4         :                
I2C_SDAT                     : H18       : bidir  : 3.3-V LVTTL       :         : 4         : Y              
oVGA_VS                      : H19       : output : 3.3-V LVTTL       :         : 4         : Y              
oVGA_R[6]                    : H20       : output : 3.3-V LVTTL       :         : 4         : Y              
oVGA_R[4]                    : H21       : output : 3.3-V LVTTL       :         : 4         : Y              
VCCA_PLL2                    : H22       : power  :                   : 1.2V    :           :                
GPIO_CLKOUT_N0               : H23       : bidir  : 3.3-V LVTTL       :         : 5         : Y              
GPIO_0[19]                   : H24       : bidir  : 3.3-V LVTTL       :         : 5         : Y              
GPIO_0[17]                   : H25       : bidir  : 3.3-V LVTTL       :         : 5         : Y              
GND*                         : H26       :        :                   :         : 5         :                
GPIO_1[2]                    : H27       : bidir  : 3.3-V LVTTL       :         : 5         : Y              
GPIO_1[4]                    : H28       : bidir  : 3.3-V LVTTL       :         : 5         : Y              
GPIO_0[14]                   : H29       : bidir  : 3.3-V LVTTL       :         : 5         : Y              
GPIO_0[15]                   : H30       : bidir  : 3.3-V LVTTL       :         : 5         : Y              
oHEX7_D[1]                   : J1        : output : 3.3-V LVTTL       :         : 2         : Y              
oHEX7_D[2]                   : J2        : output : 3.3-V LVTTL       :         : 2         : Y              
VCCIO2                       : J3        : power  :                   : 3.3V    : 2         :                
GND                          : J4        : gnd    :                   :         :           :                
GND*                         : J5        :        :                   :         : 2         :                
GND*                         : J6        :        :                   :         : 2         :                
GND*                         : J7        :        :                   :         : 2         :                
GND_PLL3                     : J8        : gnd    :                   :         :           :                
VCCD_PLL3                    : J9        : power  :                   : 1.2V    :           :                
GND                          : J10       : gnd    :                   :         :           :                
VCCIO3                       : J11       : power  :                   : 3.3V    : 3         :                
OTG_D[4]                     : J12       : bidir  : 3.3-V LVTTL       :         : 3         : Y              
iOTG_INT1                    : J13       : input  : 3.3-V LVTTL       :         : 3         : Y              
GND                          : J14       : gnd    :                   :         :           :                
VCCIO3                       : J15       : power  :                   : 3.3V    : 3         :                
VCCIO4                       : J16       : power  :                   : 3.3V    : 4         :                
GND                          : J17       : gnd    :                   :         :           :                
oI2C_SCLK                    : J18       : output : 3.3-V LVTTL       :         : 4         : Y              
oVGA_HS                      : J19       : output : 3.3-V LVTTL       :         : 4         : Y              
VCCIO4                       : J20       : power  :                   : 3.3V    : 4         :                
GND                          : J21       : gnd    :                   :         :           :                
VCCD_PLL2                    : J22       : power  :                   : 1.2V    :           :                
VCCIO5                       : J23       : power  :                   : 3.3V    : 5         :                
GPIO_0[22]                   : J24       : bidir  : 3.3-V LVTTL       :         : 5         : Y              
GPIO_0[20]                   : J25       : bidir  : 3.3-V LVTTL       :         : 5         : Y              
GND*                         : J26       :        :                   :         : 5         :                
GND                          : J27       : gnd    :                   :         :           :                
VCCIO5                       : J28       : power  :                   : 3.3V    : 5         :                
GPIO_0[16]                   : J29       : bidir  : 3.3-V LVTTL       :         : 5         : Y              
GPIO_0[18]                   : J30       : bidir  : 3.3-V LVTTL       :         : 5         : Y              
oHEX5_D[4]                   : K1        : output : 3.3-V LVTTL       :         : 2         : Y              
oHEX6_DP                     : K2        : output : 3.3-V LVTTL       :         : 2         : Y              
oHEX7_D[0]                   : K3        : output : 3.3-V LVTTL       :         : 2         : Y              
oHEX5_D[5]                   : K4        : output : 3.3-V LVTTL       :         : 2         : Y              
oHEX5_D[6]                   : K5        : output : 3.3-V LVTTL       :         : 2         : Y              
oHEX5_DP                     : K6        : output : 3.3-V LVTTL       :         : 2         : Y              
GND*                         : K7        :        :                   :         : 2         :                
GND*                         : K8        :        :                   :         : 2         :                
~nCSO~ / RESERVED_INPUT_WITH_WEAK_PULLUP : K9        : input  : 3.3-V LVTTL       :         : 2         : N              
GND_PLL3                     : K10       : gnd    :                   :         :           :                
GND                          : K11       : gnd    :                   :         :           :                
GND                          : K12       : gnd    :                   :         :           :                
VCCINT                       : K13       : power  :                   : 1.2V    :           :                
VCCINT                       : K14       : power  :                   : 1.2V    :           :                
GND                          : K15       : gnd    :                   :         :           :                
GND                          : K16       : gnd    :                   :         :           :                
VCCINT                       : K17       : power  :                   : 1.2V    :           :                
VCCINT                       : K18       : power  :                   : 1.2V    :           :                
GND                          : K19       : gnd    :                   :         :           :                
GND                          : K20       : gnd    :                   :         :           :                
GND_PLL2                     : K21       : gnd    :                   :         :           :                
GND_PLL2                     : K22       : gnd    :                   :         :           :                
GND*                         : K23       :        :                   :         : 5         :                
GPIO_0[21]                   : K24       : bidir  : 3.3-V LVTTL       :         : 5         : Y              
GPIO_0[23]                   : K25       : bidir  : 3.3-V LVTTL       :         : 5         : Y              
GND*                         : K26       :        :                   :         : 5         :                
GPIO_1[6]                    : K27       : bidir  : 3.3-V LVTTL       :         : 5         : Y              
GPIO_1[8]                    : K28       : bidir  : 3.3-V LVTTL       :         : 5         : Y              
GPIO_1[10]                   : K29       : bidir  : 3.3-V LVTTL       :         : 5         : Y              
GPIO_1[12]                   : K30       : bidir  : 3.3-V LVTTL       :         : 5         : Y              
oHEX5_D[1]                   : L1        : output : 3.3-V LVTTL       :         : 2         : Y              
oHEX5_D[2]                   : L2        : output : 3.3-V LVTTL       :         : 2         : Y              
oHEX5_D[3]                   : L3        : output : 3.3-V LVTTL       :         : 2         : Y              
iSW[15]                      : L4        : input  : 3.3-V LVTTL       :         : 2         : Y              
iSW[14]                      : L5        : input  : 3.3-V LVTTL       :         : 2         : Y              
oHEX4_DP                     : L6        : output : 3.3-V LVTTL       :         : 2         : Y              
iSW[16]                      : L7        : input  : 3.3-V LVTTL       :         : 2         : Y              
iSW[17]                      : L8        : input  : 3.3-V LVTTL       :         : 2         : Y              
GND*                         : L9        :        :                   :         : 2         :                
oDRAM1_CKE                   : L10       : output : 3.3-V LVTTL       :         : 2         : Y              
VCCIO2                       : L11       : power  :                   : 3.3V    : 2         :                
GND                          : L12       : gnd    :                   :         :           :                
VCCINT                       : L13       : power  :                   : 1.2V    :           :                
VCCINT                       : L14       : power  :                   : 1.2V    :           :                
VCCINT                       : L15       : power  :                   : 1.2V    :           :                
VCCINT                       : L16       : power  :                   : 1.2V    :           :                
VCCINT                       : L17       : power  :                   : 1.2V    :           :                
VCCINT                       : L18       : power  :                   : 1.2V    :           :                
VCCINT                       : L19       : power  :                   : 1.2V    :           :                
VCCIO5                       : L20       : power  :                   : 3.3V    : 5         :                
GPIO_0[26]                   : L21       : bidir  : 3.3-V LVTTL       :         : 5         : Y              
GPIO_0[24]                   : L22       : bidir  : 3.3-V LVTTL       :         : 5         : Y              
GND                          : L23       : gnd    :                   :         :           :                
GPIO_1[3]                    : L24       : bidir  : 3.3-V LVTTL       :         : 5         : Y              
GPIO_1[5]                    : L25       : bidir  : 3.3-V LVTTL       :         : 5         : Y              
GND*                         : L26       :        :                   :         : 5         :                
GPIO_1[9]                    : L27       : bidir  : 3.3-V LVTTL       :         : 5         : Y              
GPIO_1[7]                    : L28       : bidir  : 3.3-V LVTTL       :         : 5         : Y              
GPIO_1[14]                   : L29       : bidir  : 3.3-V LVTTL       :         : 5         : Y              
GPIO_1[15]                   : L30       : bidir  : 3.3-V LVTTL       :         : 5         : Y              
oHEX4_D[5]                   : M1        : output : 3.3-V LVTTL       :         : 2         : Y              
oHEX4_D[6]                   : M2        : output : 3.3-V LVTTL       :         : 2         : Y              
oHEX5_D[0]                   : M3        : output : 3.3-V LVTTL       :         : 2         : Y              
oHEX3_DP                     : M4        : output : 3.3-V LVTTL       :         : 2         : Y              
GND*                         : M5        :        :                   :         : 2         :                
oHEX3_D[6]                   : M6        : output : 3.3-V LVTTL       :         : 2         : Y              
oHEX3_D[5]                   : M7        : output : 3.3-V LVTTL       :         : 2         : Y              
oHEX3_D[4]                   : M8        : output : 3.3-V LVTTL       :         : 2         : Y              
oDRAM1_WE_N                  : M9        : output : 3.3-V LVTTL       :         : 2         : Y              
oDRAM1_LDQM0                 : M10       : output : 3.3-V LVTTL       :         : 2         : Y              
GND                          : M11       : gnd    :                   :         :           :                
VCCINT                       : M12       : power  :                   : 1.2V    :           :                
VCCINT                       : M13       : power  :                   : 1.2V    :           :                
VCCINT                       : M14       : power  :                   : 1.2V    :           :                
VCCINT                       : M15       : power  :                   : 1.2V    :           :                
GND                          : M16       : gnd    :                   :         :           :                
VCCINT                       : M17       : power  :                   : 1.2V    :           :                
VCCINT                       : M18       : power  :                   : 1.2V    :           :                
VCCINT                       : M19       : power  :                   : 1.2V    :           :                
GND                          : M20       : gnd    :                   :         :           :                
GPIO_0[25]                   : M21       : bidir  : 3.3-V LVTTL       :         : 5         : Y              
GPIO_0[27]                   : M22       : bidir  : 3.3-V LVTTL       :         : 5         : Y              
GND*                         : M23       :        :                   :         : 5         :                
GPIO_1[13]                   : M24       : bidir  : 3.3-V LVTTL       :         : 5         : Y              
GPIO_1[11]                   : M25       : bidir  : 3.3-V LVTTL       :         : 5         : Y              
GND*                         : M26       :        :                   :         : 5         :                
GND*                         : M27       :        :                   :         : 5         :                
GND*                         : M28       :        :                   :         : 5         :                
GPIO_1[20]                   : M29       : bidir  : 3.3-V LVTTL       :         : 5         : Y              
GPIO_1[22]                   : M30       : bidir  : 3.3-V LVTTL       :         : 5         : Y              
GND                          : N1        : gnd    :                   :         :           :                
oHEX4_D[3]                   : N2        : output : 3.3-V LVTTL       :         : 2         : Y              
oHEX4_D[4]                   : N3        : output : 3.3-V LVTTL       :         : 2         : Y              
GND*                         : N4        :        :                   :         : 2         :                
VCCIO2                       : N5        : power  :                   : 3.3V    : 2         :                
GND                          : N6        : gnd    :                   :         :           :                
oHEX3_D[3]                   : N7        : output : 3.3-V LVTTL       :         : 2         : Y              
oDRAM1_CAS_N                 : N8        : output : 3.3-V LVTTL       :         : 2         : Y              
oDRAM1_RAS_N                 : N9        : output : 3.3-V LVTTL       :         : 2         : Y              
oHEX3_D[2]                   : N10       : output : 3.3-V LVTTL       :         : 2         : Y              
VCCINT                       : N11       : power  :                   : 1.2V    :           :                
VCCINT                       : N12       : power  :                   : 1.2V    :           :                
GND                          : N13       : gnd    :                   :         :           :                
GND                          : N14       : gnd    :                   :         :           :                
GND                          : N15       : gnd    :                   :         :           :                
GND                          : N16       : gnd    :                   :         :           :                
GND                          : N17       : gnd    :                   :         :           :                
GND                          : N18       : gnd    :                   :         :           :                
VCCINT                       : N19       : power  :                   : 1.2V    :           :                
VCCINT                       : N20       : power  :                   : 1.2V    :           :                
GPIO_0[30]                   : N21       : bidir  : 3.3-V LVTTL       :         : 5         : Y              
GPIO_0[28]                   : N22       : bidir  : 3.3-V LVTTL       :         : 5         : Y              
GND*                         : N23       :        :                   :         : 5         :                
GPIO_0[31]                   : N24       : bidir  : 3.3-V LVTTL       :         : 5         : Y              
GPIO_0[29]                   : N25       : bidir  : 3.3-V LVTTL       :         : 5         : Y              
GND                          : N26       : gnd    :                   :         :           :                
VCCIO5                       : N27       : power  :                   : 3.3V    : 5         :                
GPIO_1[25]                   : N28       : bidir  : 3.3-V LVTTL       :         : 5         : Y              
GPIO_1[27]                   : N29       : bidir  : 3.3-V LVTTL       :         : 5         : Y              
GND                          : N30       : gnd    :                   :         :           :                
oHEX4_D[0]                   : P1        : output : 3.3-V LVTTL       :         : 2         : Y              
oHEX4_D[1]                   : P2        : output : 3.3-V LVTTL       :         : 2         : Y              
oHEX4_D[2]                   : P3        : output : 3.3-V LVTTL       :         : 2         : Y              
oHEX3_D[1]                   : P4        : output : 3.3-V LVTTL       :         : 2         : Y              
TCK                          : P5        : input  :                   :         : 2         :                
oHEX3_D[0]                   : P6        : output : 3.3-V LVTTL       :         : 2         : Y              
GND*                         : P7        :        :                   :         : 2         :                
TDI                          : P8        : input  :                   :         : 2         :                
oDRAM1_CS_N                  : P9        : output : 3.3-V LVTTL       :         : 2         : Y              
GND                          : P10       : gnd    :                   :         :           :                
VCCINT                       : P11       : power  :                   : 1.2V    :           :                
VCCINT                       : P12       : power  :                   : 1.2V    :           :                
GND                          : P13       : gnd    :                   :         :           :                
GND                          : P14       : gnd    :                   :         :           :                
GND                          : P15       : gnd    :                   :         :           :                
GND                          : P16       : gnd    :                   :         :           :                
GND                          : P17       : gnd    :                   :         :           :                
GND                          : P18       : gnd    :                   :         :           :                
VCCINT                       : P19       : power  :                   : 1.2V    :           :                
VCCINT                       : P20       : power  :                   : 1.2V    :           :                
GND                          : P21       : gnd    :                   :         :           :                
GND*                         : P22       :        :                   :         : 5         :                
GPIO_1[26]                   : P23       : bidir  : 3.3-V LVTTL       :         : 5         : Y              
GPIO_1[24]                   : P24       : bidir  : 3.3-V LVTTL       :         : 5         : Y              
GPIO_1[18]                   : P25       : bidir  : 3.3-V LVTTL       :         : 5         : Y              
GPIO_1[16]                   : P26       : bidir  : 3.3-V LVTTL       :         : 5         : Y              
GPIO_1[19]                   : P27       : bidir  : 3.3-V LVTTL       :         : 5         : Y              
GPIO_1[17]                   : P28       : bidir  : 3.3-V LVTTL       :         : 5         : Y              
GPIO_1[29]                   : P29       : bidir  : 3.3-V LVTTL       :         : 5         : Y              
GPIO_1[31]                   : P30       : bidir  : 3.3-V LVTTL       :         : 5         : Y              
VCCIO2                       : R1        : power  :                   : 3.3V    : 2         :                
GND+                         : R2        :        :                   :         : 2         :                
iCLK_50_4                    : R3        : input  : 3.3-V LVTTL       :         : 2         : Y              
TDO                          : R4        : output :                   :         : 2         :                
nCONFIG                      : R5        :        :                   :         : 2         :                
nCE                          : R6        :        :                   :         : 2         :                
TMS                          : R7        : input  :                   :         : 2         :                
DATA0                        : R8        : input  :                   :         : 2         :                
DCLK                         : R9        :        :                   :         : 2         :                
VCCIO2                       : R10       : power  :                   : 3.3V    : 2         :                
GND                          : R11       : gnd    :                   :         :           :                
VCCINT                       : R12       : power  :                   : 1.2V    :           :                
GND                          : R13       : gnd    :                   :         :           :                
GND                          : R14       : gnd    :                   :         :           :                
GND                          : R15       : gnd    :                   :         :           :                
GND                          : R16       : gnd    :                   :         :           :                
GND                          : R17       : gnd    :                   :         :           :                
GND                          : R18       : gnd    :                   :         :           :                
VCCINT                       : R19       : power  :                   : 1.2V    :           :                
GND                          : R20       : gnd    :                   :         :           :                
VCCIO5                       : R21       : power  :                   : 3.3V    : 5         :                
GPIO_1[30]                   : R22       : bidir  : 3.3-V LVTTL       :         : 5         : Y              
GPIO_1[28]                   : R23       : bidir  : 3.3-V LVTTL       :         : 5         : Y              
GND*                         : R24       :        :                   :         : 5         :                
GND*                         : R25       :        :                   :         : 5         :                
GPIO_1[21]                   : R26       : bidir  : 3.3-V LVTTL       :         : 5         : Y              
GPIO_1[23]                   : R27       : bidir  : 3.3-V LVTTL       :         : 5         : Y              
iCLK_50_3                    : R28       : input  : 3.3-V LVTTL       :         : 5         : Y              
iEXT_CLOCK                   : R29       : input  : 3.3-V LVTTL       :         : 5         : Y              
VCCIO5                       : R30       : power  :                   : 3.3V    : 5         :                
VCCIO1                       : T1        : power  :                   : 3.3V    : 1         :                
GND+                         : T2        :        :                   :         : 1         :                
GND+                         : T3        :        :                   :         : 1         :                
oDRAM1_A[10]                 : T4        : output : 3.3-V LVTTL       :         : 1         : Y              
oDRAM1_A[0]                  : T5        : output : 3.3-V LVTTL       :         : 1         : Y              
oDRAM1_A[1]                  : T6        : output : 3.3-V LVTTL       :         : 1         : Y              
oDRAM1_BA[0]                 : T7        : output : 3.3-V LVTTL       :         : 1         : Y              
oDRAM1_BA[1]                 : T8        : output : 3.3-V LVTTL       :         : 1         : Y              
iSW[13]                      : T9        : input  : 3.3-V LVTTL       :         : 1         : Y              
VCCIO1                       : T10       : power  :                   : 3.3V    : 1         :                
GND                          : T11       : gnd    :                   :         :           :                
VCCINT                       : T12       : power  :                   : 1.2V    :           :                
GND                          : T13       : gnd    :                   :         :           :                
GND                          : T14       : gnd    :                   :         :           :                
GND                          : T15       : gnd    :                   :         :           :                
GND                          : T16       : gnd    :                   :         :           :                
GND                          : T17       : gnd    :                   :         :           :                
GND                          : T18       : gnd    :                   :         :           :                
VCCINT                       : T19       : power  :                   : 1.2V    :           :                
GND                          : T20       : gnd    :                   :         :           :                
VCCIO6                       : T21       : power  :                   : 3.3V    : 6         :                
GND*                         : T22       :        :                   :         : 5         :                
GND*                         : T23       :        :                   :         : 5         :                
GPIO_CLKIN_P0                : T24       : input  : 3.3-V LVTTL       :         : 6         : Y              
GPIO_CLKIN_N0                : T25       : input  : 3.3-V LVTTL       :         : 6         : Y              
oSD_CLK                      : T26       : output : 3.3-V LVTTL       :         : 6         : Y              
GND*                         : T27       :        :                   :         : 6         :                
iKEY[1]                      : T28       : input  : 3.3-V LVTTL       :         : 6         : Y              
iKEY[0]                      : T29       : input  : 3.3-V LVTTL       :         : 6         : Y              
VCCIO6                       : T30       : power  :                   : 3.3V    : 6         :                
DRAM_DQ[16]                  : U1        : bidir  : 3.3-V LVTTL       :         : 1         : Y              
DRAM_DQ[17]                  : U2        : bidir  : 3.3-V LVTTL       :         : 1         : Y              
DRAM_DQ[18]                  : U3        : bidir  : 3.3-V LVTTL       :         : 1         : Y              
oDRAM1_A[2]                  : U4        : output : 3.3-V LVTTL       :         : 1         : Y              
GND*                         : U5        :        :                   :         : 1         :                
oDRAM1_A[3]                  : U6        : output : 3.3-V LVTTL       :         : 1         : Y              
oDRAM1_A[4]                  : U7        : output : 3.3-V LVTTL       :         : 1         : Y              
oDRAM1_UDQM1                 : U8        : output : 3.3-V LVTTL       :         : 1         : Y              
iSW[12]                      : U9        : input  : 3.3-V LVTTL       :         : 1         : Y              
GND                          : U10       : gnd    :                   :         :           :                
VCCINT                       : U11       : power  :                   : 1.2V    :           :                
VCCINT                       : U12       : power  :                   : 1.2V    :           :                
GND                          : U13       : gnd    :                   :         :           :                
GND                          : U14       : gnd    :                   :         :           :                
GND                          : U15       : gnd    :                   :         :           :                
GND                          : U16       : gnd    :                   :         :           :                
GND                          : U17       : gnd    :                   :         :           :                
GND                          : U18       : gnd    :                   :         :           :                
VCCINT                       : U19       : power  :                   : 1.2V    :           :                
VCCINT                       : U20       : power  :                   : 1.2V    :           :                
GND                          : U21       : gnd    :                   :         :           :                
MSEL0                        : U22       :        :                   :         : 6         :                
GND*                         : U23       :        :                   :         : 6         :                
GND*                         : U24       :        :                   :         : 6         :                
GND*                         : U25       :        :                   :         : 6         :                
nSTATUS                      : U26       :        :                   :         : 6         :                
CONF_DONE                    : U27       :        :                   :         : 6         :                
MSEL1                        : U28       :        :                   :         : 6         :                
iKEY[3]                      : U29       : input  : 3.3-V LVTTL       :         : 6         : Y              
iKEY[2]                      : U30       : input  : 3.3-V LVTTL       :         : 6         : Y              
GND                          : V1        : gnd    :                   :         :           :                
DRAM_DQ[19]                  : V2        : bidir  : 3.3-V LVTTL       :         : 1         : Y              
DRAM_DQ[20]                  : V3        : bidir  : 3.3-V LVTTL       :         : 1         : Y              
GND*                         : V4        :        :                   :         : 1         :                
VCCIO1                       : V5        : power  :                   : 3.3V    : 1         :                
GND                          : V6        : gnd    :                   :         :           :                
oDRAM1_A[5]                  : V7        : output : 3.3-V LVTTL       :         : 1         : Y              
oDRAM1_A[6]                  : V8        : output : 3.3-V LVTTL       :         : 1         : Y              
oDRAM0_LDQM0                 : V9        : output : 3.3-V LVTTL       :         : 1         : Y              
iSW[11]                      : V10       : input  : 3.3-V LVTTL       :         : 1         : Y              
VCCINT                       : V11       : power  :                   : 1.2V    :           :                
VCCINT                       : V12       : power  :                   : 1.2V    :           :                
GND                          : V13       : gnd    :                   :         :           :                
GND                          : V14       : gnd    :                   :         :           :                
GND                          : V15       : gnd    :                   :         :           :                
GND                          : V16       : gnd    :                   :         :           :                
GND                          : V17       : gnd    :                   :         :           :                
GND                          : V18       : gnd    :                   :         :           :                
VCCINT                       : V19       : power  :                   : 1.2V    :           :                
VCCINT                       : V20       : power  :                   : 1.2V    :           :                
GND*                         : V21       :        :                   :         : 6         :                
GND*                         : V22       :        :                   :         : 6         :                
GND*                         : V23       :        :                   :         : 6         :                
GND*                         : V24       :        :                   :         : 6         :                
GND                          : V25       : gnd    :                   :         :           :                
VCCIO6                       : V26       : power  :                   : 3.3V    : 6         :                
GND*                         : V27       :        :                   :         : 6         :                
GND*                         : V28       :        :                   :         : 6         :                
GND*                         : V29       :        :                   :         : 6         :                
GND                          : V30       : gnd    :                   :         :           :                
DRAM_DQ[21]                  : W1        : bidir  : 3.3-V LVTTL       :         : 1         : Y              
DRAM_DQ[22]                  : W2        : bidir  : 3.3-V LVTTL       :         : 1         : Y              
DRAM_DQ[23]                  : W3        : bidir  : 3.3-V LVTTL       :         : 1         : Y              
oDRAM1_A[7]                  : W4        : output : 3.3-V LVTTL       :         : 1         : Y              
iSW[10]                      : W5        : input  : 3.3-V LVTTL       :         : 1         : Y              
GND*                         : W6        :        :                   :         : 1         :                
oDRAM1_A[8]                  : W7        : output : 3.3-V LVTTL       :         : 1         : Y              
oDRAM1_A[9]                  : W8        : output : 3.3-V LVTTL       :         : 1         : Y              
oDRAM0_WE_N                  : W9        : output : 3.3-V LVTTL       :         : 1         : Y              
oDRAM0_CAS_N                 : W10       : output : 3.3-V LVTTL       :         : 1         : Y              
GND                          : W11       : gnd    :                   :         :           :                
VCCINT                       : W12       : power  :                   : 1.2V    :           :                
VCCINT                       : W13       : power  :                   : 1.2V    :           :                
VCCINT                       : W14       : power  :                   : 1.2V    :           :                
GND                          : W15       : gnd    :                   :         :           :                
VCCINT                       : W16       : power  :                   : 1.2V    :           :                
VCCINT                       : W17       : power  :                   : 1.2V    :           :                
VCCINT                       : W18       : power  :                   : 1.2V    :           :                
VCCINT                       : W19       : power  :                   : 1.2V    :           :                
GND                          : W20       : gnd    :                   :         :           :                
oIRDA_TXD                    : W21       : output : 3.3-V LVTTL       :         : 6         : Y              
iIRDA_RXD                    : W22       : input  : 3.3-V LVTTL       :         : 6         : Y              
oLEDG[2]                     : W23       : output : 3.3-V LVTTL       :         : 6         : Y              
GND*                         : W24       :        :                   :         : 6         :                
oLEDG[1]                     : W25       : output : 3.3-V LVTTL       :         : 6         : Y              
GND*                         : W26       :        :                   :         : 6         :                
oLEDG[0]                     : W27       : output : 3.3-V LVTTL       :         : 6         : Y              
SD_CMD                       : W28       : bidir  : 3.3-V LVTTL       :         : 6         : Y              
SD_DAT                       : W29       : bidir  : 3.3-V LVTTL       :         : 6         : Y              
GND*                         : W30       :        :                   :         : 6         :                
DRAM_DQ[24]                  : Y1        : bidir  : 3.3-V LVTTL       :         : 1         : Y              
DRAM_DQ[25]                  : Y2        : bidir  : 3.3-V LVTTL       :         : 1         : Y              
DRAM_DQ[26]                  : Y3        : bidir  : 3.3-V LVTTL       :         : 1         : Y              
oDRAM1_A[11]                 : Y4        : output : 3.3-V LVTTL       :         : 1         : Y              
GND*                         : Y5        :        :                   :         : 1         :                
GND*                         : Y6        :        :                   :         : 1         :                
oDRAM1_A[12]                 : Y7        : output : 3.3-V LVTTL       :         : 1         : Y              
oDRAM0_A[10]                 : Y8        : output : 3.3-V LVTTL       :         : 1         : Y              
oDRAM0_RAS_N                 : Y9        : output : 3.3-V LVTTL       :         : 1         : Y              
oDRAM0_CS_N                  : Y10       : output : 3.3-V LVTTL       :         : 1         : Y              
VCCIO1                       : Y11       : power  :                   : 3.3V    : 1         :                
VCCINT                       : Y12       : power  :                   : 1.2V    :           :                
VCCINT                       : Y13       : power  :                   : 1.2V    :           :                
VCCINT                       : Y14       : power  :                   : 1.2V    :           :                
VCCINT                       : Y15       : power  :                   : 1.2V    :           :                
VCCINT                       : Y16       : power  :                   : 1.2V    :           :                
VCCINT                       : Y17       : power  :                   : 1.2V    :           :                
VCCINT                       : Y18       : power  :                   : 1.2V    :           :                
GND                          : Y19       : gnd    :                   :         :           :                
VCCIO6                       : Y20       : power  :                   : 3.3V    : 6         :                
GND*                         : Y21       :        :                   :         : 6         :                
GND*                         : Y22       :        :                   :         : 6         :                
oLEDG[5]                     : Y23       : output : 3.3-V LVTTL       :         : 6         : Y              
oLEDG[4]                     : Y24       : output : 3.3-V LVTTL       :         : 6         : Y              
GND*                         : Y25       :        :                   :         : 6         :                
GND*                         : Y26       :        :                   :         : 6         :                
oLEDG[3]                     : Y27       : output : 3.3-V LVTTL       :         : 6         : Y              
FLASH_DQ[7]                  : Y28       : bidir  : 3.3-V LVTTL       :         : 6         : Y              
oFLASH_BYTE_N                : Y29       : output : 3.3-V LVTTL       :         : 6         : Y              
SD_DAT3                      : Y30       : bidir  : 3.3-V LVTTL       :         : 6         : Y              
