--------------------------------------------------------------------------------------
Timing Analyzer Summary
--------------------------------------------------------------------------------------

Type           : Worst-case tsu
Slack          : -0.396 ns
Required Time  : 1.000 ns
Actual Time    : 1.396 ns
From           : DRAM_DQ[30]
To             : Sdram_Control_4Port:sdram1|mDATAOUT[14]
From Clock     : --
To Clock       : iCLK_50
Failed Paths   : 30

Type           : Worst-case tco
Slack          : -5.418 ns
Required Time  : 1.000 ns
Actual Time    : 6.418 ns
From           : Sdram_Control_4Port:sdram1|Sdram_FIFO:write_fifo2|dcfifo:dcfifo_component|dcfifo_enm1:auto_generated|altsyncram_3731:fifo_ram|altsyncram_drg1:altsyncram3|q_a[14]
To             : DRAM_DQ[30]
From Clock     : iCLK_50
To Clock       : --
Failed Paths   : 128

Type           : Worst-case tpd
Slack          : N/A
Required Time  : None
Actual Time    : 10.587 ns
From           : iSW[3]
To             : oLEDR[3]
From Clock     : --
To Clock       : --
Failed Paths   : 0

Type           : Worst-case th
Slack          : N/A
Required Time  : None
Actual Time    : 1.608 ns
From           : GPIO_1[18]
To             : rCCD_FVAL
From Clock     : --
To Clock       : GPIO_CLKIN_N1
Failed Paths   : 0

Type           : Worst-case Minimum Pulse Width Requirement (Low)
Slack          : -1.224 ns
Required Time  : 2.127 ns
Actual Time    : 0.903 ns
From           : sdram_pll:sdram_pll0|altpll:altpll_component|_clk0
To             : Sdram_Control_4Port:sdram1|Sdram_FIFO:read_fifo1|dcfifo:dcfifo_component|dcfifo_enm1:auto_generated|altsyncram_3731:fifo_ram|altsyncram_drg1:altsyncram3|ram_block4a0~portb_we_reg
From Clock     : --
To Clock       : --
Failed Paths   : 849

Type           : Worst-case Minimum Pulse Width Requirement (High)
Slack          : -1.223 ns
Required Time  : 2.127 ns
Actual Time    : 0.904 ns
From           : sdram_pll:sdram_pll0|altpll:altpll_component|_clk0
To             : Sdram_Control_4Port:sdram1|Sdram_FIFO:read_fifo1|dcfifo:dcfifo_component|dcfifo_enm1:auto_generated|altsyncram_3731:fifo_ram|altsyncram_drg1:altsyncram3|ram_block4a0~portb_we_reg
From Clock     : --
To Clock       : --
Failed Paths   : 849

Type           : Clock Setup: 'sdram_pll:sdram_pll0|altpll:altpll_component|_clk0'
Slack          : -3.370 ns
Required Time  : 553.40 MHz ( period = 1.807 ns )
Actual Time    : 193.16 MHz ( period = 5.177 ns )
From           : Sdram_Control_4Port:sdram1|Sdram_FIFO:read_fifo1|dcfifo:dcfifo_component|dcfifo_enm1:auto_generated|dffpipe_oe9:ws_bwp|dffe6a[3]
To             : Sdram_Control_4Port:sdram1|mADDR[19]
From Clock     : sdram_pll:sdram_pll0|altpll:altpll_component|_clk0
To Clock       : sdram_pll:sdram_pll0|altpll:altpll_component|_clk0
Failed Paths   : 9600

Type           : Clock Setup: 'iCLK_50'
Slack          : 1.195 ns
Required Time  : 166.00 MHz ( period = 6.024 ns )
Actual Time    : 207.08 MHz ( period = 4.829 ns )
From           : Reset_Delay:reset0|Cont[28]
To             : Reset_Delay:reset0|oRST_0
From Clock     : iCLK_50
To Clock       : iCLK_50
Failed Paths   : 0

Type           : Clock Setup: 'GPIO_CLKIN_N1'
Slack          : 1.776 ns
Required Time  : 110.01 MHz ( period = 9.090 ns )
Actual Time    : 136.72 MHz ( period = 7.314 ns )
From           : CCD_Capture:capture0|Y_Cont[6]
To             : RAW2RGB:rgb0|rGreen[10]
From Clock     : GPIO_CLKIN_N1
To Clock       : GPIO_CLKIN_N1
Failed Paths   : 0

Type           : Clock Setup: 'vga_pll:vga_pll0|altpll:altpll_component|_clk0'
Slack          : 2.960 ns
Required Time  : 108.00 MHz ( period = 9.259 ns )
Actual Time    : 158.76 MHz ( period = 6.299 ns )
From           : VGA_Controller:vga0|V_Cont[1]
To             : VGA_Controller:vga0|oVGA_R[4]
From Clock     : vga_pll:vga_pll0|altpll:altpll_component|_clk0
To Clock       : vga_pll:vga_pll0|altpll:altpll_component|_clk0
Failed Paths   : 0

Type           : Clock Hold: 'iCLK_50'
Slack          : -1.932 ns
Required Time  : 166.00 MHz ( period = 6.024 ns )
Actual Time    : N/A
From           : I2C_CCD_Config:i2c0|senosr_exposure[7]
To             : I2C_CCD_Config:i2c0|mI2C_DATA[7]
From Clock     : iCLK_50
To Clock       : iCLK_50
Failed Paths   : 108

Type           : Clock Hold: 'sdram_pll:sdram_pll0|altpll:altpll_component|_clk0'
Slack          : 0.391 ns
Required Time  : 553.40 MHz ( period = 1.807 ns )
Actual Time    : N/A
From           : Sdram_Control_4Port:sdram1|command:command1|do_rw
To             : Sdram_Control_4Port:sdram1|command:command1|do_rw
From Clock     : sdram_pll:sdram_pll0|altpll:altpll_component|_clk0
To Clock       : sdram_pll:sdram_pll0|altpll:altpll_component|_clk0
Failed Paths   : 0

Type           : Clock Hold: 'vga_pll:vga_pll0|altpll:altpll_component|_clk0'
Slack          : 0.391 ns
Required Time  : 108.00 MHz ( period = 9.259 ns )
Actual Time    : N/A
From           : VGA_Controller:vga0|mVGA_V_SYNC
To             : VGA_Controller:vga0|mVGA_V_SYNC
From Clock     : vga_pll:vga_pll0|altpll:altpll_component|_clk0
To Clock       : vga_pll:vga_pll0|altpll:altpll_component|_clk0
Failed Paths   : 0

Type           : Clock Hold: 'GPIO_CLKIN_N1'
Slack          : 0.391 ns
Required Time  : 110.01 MHz ( period = 9.090 ns )
Actual Time    : N/A
From           : CCD_Capture:capture0|mCCD_FVAL
To             : CCD_Capture:capture0|mCCD_FVAL
From Clock     : GPIO_CLKIN_N1
To Clock       : GPIO_CLKIN_N1
Failed Paths   : 0

Type           : Other violations (see messages)
Slack          : 
Required Time  : 
Actual Time    : 
From           : 
To             : 
From Clock     : 
To Clock       : 
Failed Paths   : 2

Type           : Total number of failed paths
Slack          : 
Required Time  : 
Actual Time    : 
From           : 
To             : 
From Clock     : 
To Clock       : 
Failed Paths   : 11566

--------------------------------------------------------------------------------------

